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Nonstructural Component Checklist
The attached checklist must be provided near the front of the construction plans of all DFCM projects involving new construction, building additions, or the addition of new or replacement components.  One box must be checked within each row.  Comments should be provided noting the particular component(s) that require seismic restraint.  
Review the “DFCM Guidelines for Seismic Restraint of Nonstructural Components” document for clarification on the requirements for non-structural components and an example of how to fill out the attached checklist. 
Notes:

1. Deferred submittals for seismic restraint of nonstructural components must be submitted to the DFCM Building Official a minimum of two weeks prior to the planned installation in order to allow for plan review and forwarding to inspectors.  In the event that the submittal is deficient additional time may become necessary. 

2. When seismic restraint of non-structural components is installed prior to receiving DFCM approval it shall not be covered or concealed until receiving both plan review and inspection approval.  Further, installers are proceeding at their own risk until plan review and inspection approval occurs. 

3. The requirements for seismic restraint of nonstructural components cannot be satisfied by a general reference to Design Manuals.  The design professional may utilize these manuals as a basis of their design, but must provide all supporting documentation to ensure that the design conforms to the requirements of ASCE 7-05, Chapter 13.

4. Submittals must include details of the proposed seismic restraint of nonstructural components.  These details must show specific information relating to the materials, type, size, and locations of anchorages; materials used for bracing; attachment requirements of bracing to structure and component; and locations of transverse and longitudinal sway bracing and rod stiffeners. Submittals may also require structural calculations, engineering reports, test data, and/or specifications to ensure code compliance.   

	DFCM NONSTRUCTURAL COMPONENT CHECKLIST

	ITEM DESCRIPTION
	NOT REQUIRED
	ON CONST. DOCUMENTS
	DEFERRED SUBMITTAL
	COMMENTS

	Architectural Components:

	Interior Nonstructural Walls & Partitions
	
	
	
	

	Cantilever Elements (i.e. parapets, etc.)
	
	
	
	

	Exterior Nonstructural Wall Elements
	
	
	
	

	Veneer
	
	
	
	

	Penthouses
	
	
	
	

	Ceilings (i.e. suspended grid or hard lid)
	
	
	
	

	Cabinets (i.e. storage cabinets, equipment, etc.)
	
	
	
	

	Access Floors
	
	
	
	

	Storage Racks
	
	
	
	

	Appendages & Ornamentations
	
	
	
	

	Signs & Billboards
	
	
	
	

	Other:
	
	
	
	

	Other:
	
	
	
	

	MEP Components:

	Fire Sprinklers
	
	
	
	

	Mechanical Equipment (i.e. HVAC, fans, air handlers, boilers, furnaces, tanks, chillers, water heaters, heat exchangers, evaporators, engines, turbines, pumps, compressors, MFR equipment, etc.)
	
	
	
	

	Electrical Equipment (i.e. generators, batteries, inverters, transformers, MCC, panel boards, switch gear, cabinets, etc.)
	
	
	
	

	Elevator & Escalator Components
	
	
	
	

	Communication Equipment, Computers, Instrumentation, and Controls
	
	
	
	

	Roof-mounted Chimneys, Stacks, Cooling & Electrical Towers
	
	
	
	

	Lighting Fixtures
	
	
	
	

	Vibration Isolated Components
	
	
	
	

	Piping & Conduit Systems
	
	
	
	

	Ductwork (including in-line components)
	
	
	
	

	Conveyors
	
	
	
	

	Cable Trays
	
	
	
	

	Other:
	
	
	
	

	Other:
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